RED Guide Creator     v1.0.11        March 31, 2017

########################################################################################
Overview
The REDGuideCreator and REDKeyMapper applications empower you to create, edit, and customize your 
DSMC projects and DSMC function buttons from a convenient visual interface on a computer. 

########################################################################################
Equipment Requirements  
DSMC BRAIN          SCARLET, EPIC, or DRAGON with firmware v4.x or higher
Operating System    Windows XP or higher
                    OSX 10.6 or higher  
Hard drive space    30MB (Windows, for both applications)
                    102MB (OSX, for both applications)
########################################################################################
Installation on Mac

1. Download the “DSMC Resources” package from the RED downloads page.
2. Unzip the “DSMC Resources” zip file.
3. Locate the RED application .dmg file in the “Mac” folder.
4. Double-click the .dmg file to mount the installer.
5. Click and drag the application icon to the Applications folder.
6. Locate the application in the Applications folder.
7. Right-click on the application and select Open.
8. Select OK to approve.

Installation on PC

1. Download the “DSMC Resources” package from the RED downloads page.
2. Unzip the “DSMC Resources” zip file.
3. Locate the RED application file in the “Win” folder.
4. Double-click on the file and select Run. 
5. Click the “I Agree” button.
6. Choose a destination folder for install. Select Next.
7. Select Install.
 
########################################################################################
REDKeyMapper Controls and Operations

The REDKeyMapper allows you to create, edit, and customize DSMC function buttons on your DSMC BRAIN and modules. 
Use this application to make changes to the mapped DSMC key functions. The REDKeyMapper includes the following 
application elements.

Navigation bar      Access DSMC component tabs along the top of the application. 
Component tabs      Open component-specific windows for function adjustment.
Remove button       Click to remove all mapped actions for this key function.
Edit button         Click to open the Key Mapping Menu.
Key Mapping menu    Adjust or fully customize camera button functions.
Dropdown menu       Select the desired action from this picking list.
Action checkbox     This box automatically checks when key function is mapped or active. 
                    Uncheck this box to remove the mapped key function.

Set a Button Function

1. Select the desired component tab from the navigation bar.
2. Click on the EDIT button to open the Key Mapping menu.
   Alternatively, hover over the function in the image to highlight it. Click on the red highlighted function.
3. Click on the dropdown menu to show action options.
4. Select the desired action from the dropdown menu.
5. Select OK when finished.

Remove a Button Function

1. Select the desired component tab from the navigation bar.
2. Click on the EDIT button to open the Key Mapping menu.
   Alternatively, hover over the function in the image to highlight it. Click on the red highlighted function. 
3. Click on the action checkbox to uncheck it. This removes the mapped action.
4. Select OK when finished.

Note: Alternatively, from the component tab, click on the REMOVE button to remove all mapped actions for the specific key function.
Note: For more information, see the DSMC Operation Guide available at red.com/downloads.

########################################################################################
REDGuideCreator Controls and Operations

The REDGuideCreator allows you to create, edit, and customize your DSMC project and overlay presets. 
Use this application to adjust DSMC UI and project settings. The REDGuideCreator consists of the following 
Application elements:

Project Settings        Choose your specific DSMC sensor and project format. 
Frame Guide             Adjust the appearance of your DSMC frame guide, action guide, and title guide.
General Settings        Adjust various elements of your DSMC UI. 

Change the Firmware Version of a Preset

Due to the nature of DSMC firmware, the version must be selected prior to creating the preset file. Because 
of this, you cannot change a preset firmware version once you have started the preset creation process. Create 
a new preset and configure the desired settings.

Note: For more information, see the DSMC Operation Guide available at red.com/downloads.

########################################################################################
General Operations

Configure a Preset with Settings from both Applications

A preset can be created and configured with either of the applications. Follow these steps to create a preset 
with settings from both REDGuideCreator and REDKeyMapper.
1. Create and configure a preset using the REDGuideCreator application.
2. Save the preset and close the application.
3. Open the REDKeyMapper application. 
4. Select Open when prompted. 
5. Locate and open the .preset file that was just created.
6. Configure preset as desired
7. Once you are completed, save the preset. The preset now includes settings from both applications.

Save Presets to a RED SSD

Once you are finished configuring the preset, you need to save the preset to a RED media device (SSD).
1. Connect the appropriate RED STATION, for your REDMAG or RED MINI-MAG, to your computer.
2. Insert/Mount a formatted RED SSD.
3. Place the saved preset file into the “Presets” folder on your RED SSD. If there is not a "Presets" 
folder on the SSD, create one now.
4. Properly eject the RED SSD, and remove the RED SSD from the RED STATION.
Note: The preset file must be saved in a folder labeled “Presets” on the RED SSD. If it is not, the camera will 
not recognize the preset file.

Load Presets to DSMC

Once you have saved and loaded the desired presets to a RED SSD, follow these steps:
1. Insert the formatted RED SSD into your DSMC.
2. Navigate to the Presets menu on the camera, Menu > Presets > Camera Presets.
3. From the Camera Presets menu, select the desired preset to load from the “S-SSD/presets” box on the right.
4. Press the “?” button in the middle.
    Alternatively, press the “? All” button in the middle to load all presets on the RED SSD.
5. When prompted “Would you like to apply the imported preset”:
    Choose YES to apply the preset now.
    Choose NO to apply the preset at a later time.

########################################################################################
Significant changes since previous build:
* Added v6.4 support


Operational notes:
* None

Copyright (c) 2017 RED Digital Cinema, All Rights Reserved.