Epic, Scarlet and Dragon Preset Files		April 13, 2015

The procedure will apply a preset file to the camera on startup.

1) Insert a formatted SSD MAG into the REDstation and creata a 'force_preset' folder
2) Unzip the file and locate the required preset file.
3) Copy the required preset file to the 'force_preset' folder. 

NOTE: Ensure you have selected a file from the correct camera version folder.

4) With the camera OFF, install the SSD Mag and power up the camera.
5) The camera will recognize the preset file, apply it and delete the folder.




